Generator, Irrigation equipment material for Ntabankulu Farm project (ward 08) Installation (labour) and also deliver to the site as per specification:-

|  |  |
| --- | --- |
| **Description** | **Quantity**  |
| **Revive Irrigation scheme**  |  |
| HDPE PIPE PE 100 40 MM PN 1040 MM HDPE PN 10 SDDR17 100M | 200 |
| PIPE RISER HDPE 25MM XO,600MET | 17 |
| COMP END CAP 40MM | 1 |
| COMP COUPLING 40MM | 1 |
| COMP TEE 40MM | 1 |
| BRASS BALL GATE VALVE 40MM | 1 |
| COMP ADAPTOR MALE 40X40MM M ADAPTOR 40 11/2’’ | 2 |
| HYDROMATIC PVC ORANGE BENSKON NYLOMATIC WITH SPRING  | 17 |
| ALUM PLASTIC BLK 20PIPLET PLUSTIC BLK  | 17 |
| HOSE CLAMP 12MMCLAMP HOSE GS 12 | 34 |
| DRAGLINE HOSE 5YR 20MM | 1224 |
| DRAGLINE STAND 20MM | 34 |
| NORMAC TWIN DIESIL PUMP  | 1 |
| HELIFLEX 40MM | 6 |
| COUPLING FEM/FEM11/2’’ | 2 |
| M ADAPT /HOSE 40MM | 1 |
| COMP ADAPTOR MALE 40X40MMM ADAPTOR 40M11/2’’ | 1 |
| GALV BEND M/F 40MM | 1 |
| COMP SADDLE 40X25MM | 17 |

**SPECIFICATION**

 **DEVELOPMENT PLANNING**